**If you can’t be without your licence, know your limit and your options with a quick test.**



[Stealth Professional Breathalyser](http://breathalyzersonline.com.au/p42-New-Alcosense-AL9000-Stealth-L-Breathalyzer.html)

Fuel Cell Breathalyser

Sleek, small and accurate. Latest technology, stylish, lightweight design.

**\*Electrochemical fuel cell sensor - high accuracy and reliability.**

**\*Australian Standard AS3547 Certified \* Accuracy +/- 0.005% BAC at 0.100%BAC**

**\*High accuracy with 3-decimal reading \* Ideal for accurate personal use**

**\*Indication of B.A.C 0.000 to 0.400%BAC (Full 3 decimals)**



Portable Charging Breathalyser

Features accurate fuel cell sensor, rechargeable battery and also functions as a portable charging station. Practical and multifunctional breathalyser that is a must-have for those who are always on-the-go.

**\*Rechargeable internal battery \* Last reading recall, temperature and flashlight**

**\*Supercharge your social life! \* Highly accurate 3-decimal place**

**\* Portable charging station for mobile phones & cameras**



Corporate “Z” Breathalyzer

Perfect for on the go. Compact, lightweight, easy to use, with data-saving capabilities.  **\*Highly accurate hand-held device for personal and professional use**

**\*Easily replaced recalibrated sensor \*Low battery indication**

**\*BAC Range: 0.000~0.400% BAC. \*Accuracy: +/- 0.010% BAC.**

**\*Audible alert when alcohol detected.**

 [PRO 2013 Professional](http://breathalyzersonline.com.au/p3-Andatech-AL6000PRO-Professional-Silver.html)

World first breathalyser that can be operated in dual-mode; it can be operated in a normal mode

to measure specific blood alcohol concentration, or it can be used as an alcohol responder

**\* Certified Australian Standard AS3547 \* Perfect for professional and personal use**

**\*Accuracy: +/- 0.010% at 0.050% BAC \* 12 Month Manufacturer’s Warranty**

**\* New oxide semiconductor-type alcohol sensor**



[Elite 2013 Breathalyser](http://breathalyzersonline.com.au/p23-AlcoSense-Elite-II-Breathalyzer.html)

Simple to use. Microcomputer-controlled automatic test sequence with a 2 decimal LCD display, audible warnings on the detection of alcohol. Exceptionally light, conveniently sized, easy storage.

**\*Accurate hand-held device \*Breath flow check**

**\*Sensor Type New Oxide Semiconductor \*Indication of BAC0.00% to 0.4% BAC**

**\*Warranty 6 Months**